**Natural light controls and guides in buildings. Energy saving for electrical lighting, reduction of cooling load**

**E.J. Gagoa\*, T. Muneer**b**, M. Knez**c**, H. Kösterd**

aSchool of Civil Engineering, University of Granada, Granada, Spain

**b**School of Engineering and Built Environment, Edinburgh Napier University, Edinburgh, Scotland, UK

c Faculty of logistics, University of Maribor, Maribor, Slovenia

d Köster Lichtplanung, Karl-Bieber Höhe 15, D-60437 Frankfurt, Germany

*\*Corresponding author: Tel: +34 958 24 13 51. Fax: +34 958 24 27 15. Email address:* *ejadraque@gr.es*

**Abstract**

The residential sector is responsible for approximately a quarter of energy consumption in Europe. This consumption, together with that of other buildings, mainly from the tertiary sector, makes up 40% of total energy consumption and 36% of CO2 emissions. Artificial lighting makes up 14% of electrical consumption in the European Union and 19% worldwide. Through the use of well-designed natural lighting, controlled by technologies or systems which guarantee accessibility from all areas inside buildings, energy consumption for lighting and air conditioning can be kept to a minimum. The authors of this article carried out a state of the art on the technologies or control systems of natural light in buildings, concentrating on those control methods which not only protect the occupants from direct solar glare but also maximise natural light penetration in buildings based on the occupants’ preferences, whilst allowing for a reduction in electrical consumption for lighting and cooling. All of the control and/or natural light guidance systems and/or strategies guarantee the penetration of daylight into the building, thus reducing the electrical energy consumption for lighting and cooling. At the same time they improve the thermal and visual comfort of the users of the buildings. However various studies have also brought to light certain disadvantages to these systems.

**Keywords:** sustainable building, healthy buildings, environmental impact of daylight and control systems of daylighting.

* + - 1. **Introduction**

The residential and tertiary sector, makes up 40% of total energy consumption [1,2,3,4,5,6,7,8] and 36% of CO2 emissions [9]. According to the International Energy Agency (IEA) [10], artificial lighting makes up 14% of electrical consumption in the European Union and 19% worldwide.

By acting on energy efficiency in buildings, it is possible to reduce energy consumption and therefore CO2 emissions into the atmosphere [11,12]**.** Lancashir et al. [13] reported that each kWh of energy saved prevents the emission of 680.39 g of carbon dioxide, 5.67 g of sulphur dioxide, and 2.27 g of nitrogen oxide.

Many studies have been able to demonstrate the importance of natural light in buildings. Natural light significantly influences both the balance of energy use in buildings and actual human activity [14,15,16,17], offering the occupants comfort and health benefits, given that it plays an important biological role in the control of the physiological and psychological rhythms of living beings [18,19,20]**.**

However, due its changing nature, it is necessary to control and guide natural light in order to supplement or replace artificial lighting. If it is not controlled, natural light can have a negative impact on the environment as excessive solar gains lead to an increase in energy consumption for cooling. On the other hand, most natural light control systems concentrate on minimizing the negative impact of natural light, whilst ignoring its positive impact. Through aiming to reduce the external heat load caused by solar radiation in a building, the amount of natural light often becomes insufficient and results in an increase in energy used for electrical lighting [21]**.** Thus, for example, windows allow daylight to enter into and illuminate the interior of a building, yet the effects of the natural light decrease as one moves away from the windows, making the use of artificial illumination a necessary complement [22]**.**

Therefore, through a well-designed, controlled use of natural light, employing technologies or systems which ensure the penetration of light throughout the whole building, energy consumption designated to lighting and air conditioning can be kept at a minimum [23,24,25,26,27,28,29,30,31,32,33,34,35]**.**

The authors of this article carried out a state of the art on the technologies or control systems of natural light in buildings. The efficiency of each of these systems in the reduction of energy consumption was evaluated. Specifically, the research concentrates on those control methods which not only protect the occupants from direct solar glare but also maximise daylight penetration into buildings based on the occupants’ preferences, whilst allowing for a reduction in electrical consumption given over to lighting and cooling.

* + - 1. **Impact of control systems of natural light**

Electric lighting energy consumption [kWh] in conventional office buildings is as much as 35% of the total electric load - demands that are generated primarily during the day when daylight is abundant. Since the energy drawn for electric lighting is ultimately converted into heat, there is additionally a load on the cooling system. Proportional to the total energy used, electric lighting can add as much as 16% to the cooling energy bill, such that the combined electricity costs for lighting and cooling are almost 50% of total electric demand. While total energy consumption is made up of both electricity and fossil fuel energy uses, daylighting alone can reduce total energy use by as much as 25-30%, one of the most cost-effective investments for energy and carbon savings world-wide [21].

The economic impact of ignoring daylight is even more problematic because it is an electric load in buildings – for which source or primary energy costs are significant. 1kW of power on site uses approximately 3-4kW of primary energy, with the rest lost as heat up the chimney at the power plant. In conventional coal or oil fired power plants, only 35-40% of the primary energy is converted into power with a further 6% of the energy produced at the power plant lost in transmission. In developed economies such as the USA, Japan, Germany, power plants are to blame for approximately 50% of all CO2 emissions. Over 40% of each nation’s total energy consumption in developed economies is used for heating, cooling, air conditioning, lighting and other power requirements in buildings [21].

In addition, the benefits of a daylight building extend beyond simple energy savings [36,37]. Numerous studies also indicate that daylighting can help increase worker productivity and decrease absenteeism in daylight commercial office buildings, boost test scores in daylight classrooms [38], and accelerate recovery and shorten stays in daylight hospital patient rooms. Hourani and Hammad [39] reported impacts of daylight on students’ health, emotions, attendance and performance. A 2 year study in U.S. elementary schools cleared more attendance by 3.6% for students in daylight classes than students in other classes depend mainly on electrical lighting and minimum day-lighting. Another study in U.S. schools investigated the impact of daylight on students’ performance through scores’ analysis for over (21,000) students. Whereas students in the most daylight classrooms showed progress 20% faster on math tests and 26% on reading tests within 1 year than students in classes depending on electrical lighting with minimum daylight [39].

* + - 1. **Daylighting legislation**

There are many types of building regulations, codes, standards or ordinances which are specifically related to ensure daylight in buildings. The requirements and regulations regarding daylight are very diverse. The existing daylighting standards in many European countries (comprehensive codes are for example in Germany [40] and Great Britain [41]) are more or less informative and are not intended to be applied in a prescriptive manner. The European Committee for Standardization will prepare the first European Code for daylighting in buildings and to define metrics for daylight and sunlight in all regularly occupied indoor spaces [42].

A good review of daylighting requirements of many sustainable rating systems was done in Ref. [43].

* + - 1. **Selection of research studies**

This paper systematically reviews recent research on the technologies or control systems of natural light in buildings. The main objective of such technologies or control systems is not only to protect occupants from direct solar glare but also maximize daylight penetration into buildings based on occupants’ preferences, whilst allowing for a reduction in electrical consumption for lighting and heating. The methodology used for this systematic review is described in [44] and [45], and consists of the following steps:

* Exhaustive search of the literature by applying pre-defined criteria for the identification of the most relevant articles in the field.
* Critical evaluation of the quality of the selected articles by synthesizing their content and summarizing the results and conclusions.

For this research, the data were obtained by searching databases of different disciplines (e.g. environmental and daylighting studies and public health). The search engines used were those on Internet, environmental and daylighting web pages. The key words for the searches were daylighting, sustainable building, healthy buildings and environmental impact of daylight and control systems of daylighting. The inclusion criteria for articles were explicitly defined in consonance with the characteristics of the study. To be included in the review, the article had to be an in-depth study of daylighting, its characteristics, influential factors, consequences, technologies or control systems, effects on human health and environment, etc.

The structure of this review reflects the inventory of possible control systems of daylighting in buildings. These control systems were identified by analyzing the contents of the articles. The articles analyzed in the review were retrieved from the following data bases: [Journal Citation Reports, [Web of Knowledge, Web of Science, and](http://biblioteca.ugr.es/pages/biblioteca_electronica/bases_datos/web-of-knowledge) Scopus](http://biblioteca.ugr.es/pages/biblioteca_electronica/bases_datos/journal-citation-reports-sciences). From each article, the research objectives, the description of the methodology applied or developed, the geographical location of the study, theoretical premises, computer tools used, and above all, the information in the conclusions regarding the technologies or control systems of daylighting in buildings were extracted.

* + - 1. **Natural light controls and light guides in buildings**

According to the International Energy Agency (IEA) [10], artificial lighting makes up 14% of electrical consumption in the European Union and 19% worldwide.

There is a great variety of systems to control and/or guide the natural light which penetrates the interior of a building, put in place with the aim of reducing energy consumption. These systems or strategies of control and/or guidance of natural light can be divided into two groups:

* Side-lighting systems
* Top-lighting systems

The first group includes systems of lateral illumination where natural light enters the interior of a building through the sides. A window is the simplest example of this group of systems or strategies. Zain-Ahmed et al. [46]presented a study on energy savings achieved through the use of daylight in passive solar building design. They proved that by modifying the size of the windows, a minimum saving of 10% in electrical energy consumption is achieved.

In the second group, natural light enters the interior of a building from the top. A skylight would be the simplest example of this group.

The main objective of these systems and/or strategies of control and/or guidance of natural light is not only to maximize levels of natural light inside a building but also optimize the light quality in the environment for its occupants (an excess of natural light can be uncomfortable). The key to well-designed natural illumination lies in the control, not only of levels of light, but also in the direction and distribution of the light. In this way both the comfort of the occupants and the reduction in electrical energy consumption for lighting [47]and cooling [48]will be assured.

* 1. **Side-lighting systems**

Side-lighting systems are designed to avoid an unequal distribution of natural light which may occur through the use of traditional lateral windows. These systems achieve a more uniform, balanced distribution of natural light inside a building through the reduction of excessive levels of light near the windows and an increase in the light in areas situated far from the windows. In this article the side-lighting systems analysed are:

* Light shelves
* Prismatic glazing
* Mirrors and holograms
* Anidolic ceiling
* Louvres and blinds
	+ 1. **Light shelves**

Light shelves are components placed horizontally in a window above eye level. As Ochoa and Capeluto [49]demonstrate, these systems protect the lower areas near a window from direct solar radiation. They also reduce the contrast between the light levels generated in the vicinity of the window and those at the back of the room. Edmonds and Greenup [50] showed that light shelves are a good device for shading and natural lighting.

Light shelves are divided into superior and inferior sections. Their job is to reflect the light which shines on them towards the surface of the ceiling in order to achieve a better penetration and more uniform distribution of light, whilst decreasing the electrical energy consumption for lighting. In this way Sanati and Utzinger [51] showed that spaces where the windows had been fitted with light shelves used less electricity for lighting than those with conventional windows.

As these systems operate by reflecting the light which falls upon them towards the surface of the ceiling, the geometry of both the ceiling and the light shelves plays a very important role in their performance. Freewan et al. [52], proved that the best ceiling is one which is curved in both the front and the rear of the room. In a subsequent study the authors analysed the interaction between the different geometries of the light shelves when combined with a curved roof, finding the best light shelves are curved and bevelled [53]. Al-Sallal [54] revealed that a roof pitch of 5º contributes to a reduction in the difference in brightness between the ceiling and the back wall.

Light shelves affect the architectural and structural design of a building and must be considered at the beginning of the design phase as they require a specific roof type in order to function efficiently. Light shelves must be designed specifically for every window orientation, room configuration or latitude [55,56]. Although light shelves are only effective during the seasons of the year where light falls directly onto them, they help reduce glare. As they reduce levels of illumination they are not always apt for rooms with north exposure [49].

* + 1. **Prismatic glazing**

Devices similar to prismatic glazing have been used for many years to adapt daylight in such a way so that the diffused solar radiation enters into a building whilst the direct radiation is reflected [57]. Critten [58] showed that prismatic glass could be used to enhance winter sunlight in greenhouses, whilst Kurata [59]demonstrated the effects of a Fresnel prism in a greenhouse cover, concluding that the transmission of light in winter was increased whilst in summer it decreased.

Prismatic glazing follows the basic laws of reflection and refraction of sunlight to change the inbound direction of the light and redistribute it. Part of the incidental sunlight is reflected on the ceiling while the rest stays near the window. In this way a better penetration and more uniform distribution of sunlight can be achieved [60]. Lorenz [61]proved that this heightened penetration and uniformity of light reduces electrical energy consumption for cooling as it offers a significant improvement in the thermal comfort of the users during the summer months. Along these lines, Christoffers [62]managed to reduce electrical energy consumption for cooling and heating by decreasing the direct solar radiation falling onto the front of a building by 10% in the summer whilst transmitting 90% of this radiation in winter.

Various studies have concentrated on different aspects of prismatic glazing, with the objective of improving the distribution of daylight inside rooms [63,64]. Some of the aspects which have been analysed include: design, thickness, deviation angle, amount of deviated light…

However, the effect of prismatic glazing when the sky is overcast is negligible. In this case the prismatic plates are placed between two transparent panes of glass at the top of the window. Along these lines Edmonds [65], analysed a material of a similar thickness to conventional glass windows, with a prismatic glazed laminate placed between two panes. The resulting material offered a more efficient distribution of sunlight.

Insert Figure 1

* + 1. **Mirrors and holograms**

Mirrors and holographic sheets or HOEs (Holographic Optical Elements) allow a redirection of natural light, improving light penetration and distribution inside buildings [60]. Both systems offer large potential savings in energy and improved comfort for users [66]. Breitenbach and Rosenfeld [67]investigated the optical properties of holograms, concluding that, as they separate the majority of the light visible from the infrared part of the solar spectrum, they are an efficient means of both controlling natural light and optimizing sunlight gain.

Various authors have studied the environmental advantages of holograms. Müller [68]proved that through the use of holograms, electrical consumption for lighting could be reduced by more than 50% when complemented with an automatic control system for the lights. James and Bahaj [69] showed that the temperature in a greenhouse could be reduced by as much as 6.1 degrees if holograms were added to 62% of the glass.

However, according to Tholl et al. [70], holograms offer the disadvantage of reducing transparency in an environment whilst Klammt et al. [71]state that the high cost of holograms means that using them on a large scale is difficult. Furthermore Köster [21]concludes that mirror glass windows reduce the transmission of energy through the glazed surface. This means that, by reducing the external heat load resulting from solar irradiation into the building being reflected and/or absorbed in the outer skin, energy use for electric lighting is increased (Figure 2).

Insert Figure 2

* + 1. **Anidolic ceilings**

The anidolic ceiling is a system which offers an improvement not only in the levels of natural light inside a building but also in energy efficiency [72,73]. Wittkopf et al. [74]proved that more than 20% of electrical energy consumption for lighting could be saved using this system. For Courret et al. [75]this saving inelectrical energy for lighting is 30%. Using a comparative study, these authors proved furthermore that personal appreciation of the luminous atmosphere is higher in a room with an anidolic ceiling, leading to a significant reduction in reading errors both on paper and on the screen. Scartezzini and Courret [76]showed that on an overcast day, thedaylight factor, measured at the back of a room, increased by 1.7; this allows for a reduction in electrical energy consumption for lighting of a third. Furthermore, measurements of visual comfort recorded that, with an overcast sky, the anidolic ceiling offers better quality illumination than conventional glazing. Linhart and Scartezzini [77] proved that with anidolic lighting systems, lighting power densities can be reduced by at least 4 W/m2 with no significant impact on visual comfort and efficiency; even a 3 W/m2 reduction is a realistic possibility.

Vázquez-Moliní et al. [78], describe in detail the anidolic collecting system as a part of the comprehensive daylighting system. The day lighting system is based on a T-CPC (runcated Compound Parabolic Concentrator) collection system that minimizes the system’s dependence on solar incidence which means an appropriate behavior for virtually any time of year during working hours. Moreover the controlled aperture angle, limited by the collector array, reduces reflection losses.

Other authors such as Ochoa and Capeluto [49] proved that the anidolic ceiling offers high levels of illumination in quantitative terms. However, qualitatively, care must be taken over solar angles where the reflection hub may cause glare. Errors in the size or orientation of the hub may cause undesired reflections, even when the system’s performance is good.

* + 1. **Louvres and blinds**

Louvres and blinds are two systems designed to capture the sunlight entering into the front part of a room and redirect it towards the back. This increases light levels at the back of the room whilst reducing them at the front.

Insert Figure 3

Louvres and blinds are made up of numerous horizontal, vertical or sloping slats. Due to the discreet nature of the device, its optical (and thermal) properties are complex and depend on several parameters including louvre characteristics, tilt angle and solar angle of incidence. Rotation angle, shape, size, configuration and colour of slats all have an impact on glare and visibility, but also on effective transmittance, absorption and reflectance of a window-blind system [79]**.**

Much of the research carried out on louvres and blinds concentrates on calculating their optical properties and other questions relating to their control, employing experimental techniques [80,81,82], analytical models [83,84,85], semi-analytical and numerical methods [86,87,88,89] and ray-tracing simulation [90,91,92]**.**

Numerous authors have studied the influence of louvres and blinds on electrical energy consumption in buildings. Along these lines, Hammad and Abu-Hijleh [93]examined the changes in electrical consumption in an office block situated in Abu Dhabi, in the United Arab Emirates. They compared this system with another, simpler method of using light dimmers controlled by a sensor. The results showed that the potential energy savings when using the dimmers was merely 24.4%, 24.45% and 25.19% in the south, east and west-facing facades, respectively. The proposed system of dynamic blinds together with the gradual light reduction strategy meant energy savings of 34.02%, 28.57% and 30.31% in a southern, eastern and western orientation, respectively. Saelens et al. [94]evaluated the influence on cooling demands and the peak cooling potential of a south-facing office when different models and perspectives were applied to simulate performance of external Louvre shading devices.

Oh et al. [95] optimized control strategies of slat-type blinds through two stages. In the first stage, double-sided blinds were suggested by applying different reflectance between the front and back of the slat and by fully rotating the slat when the system mode was switched between heating and cooling. When the double-sided blind was used alongside the controlled light dimmers, an energy saving of 24.6% could be achieved when compared to the baseline case, and simultaneously glare could be avoided. In the second stage, the control strategies of slat angle and up/down control logic were developed to fully remove glare and improve the energy efficiency. As a result, an energy saving of 29.2% could be achieved whilst glare was reduced to just 0.1%. Shen et al. [96], evaluated and compared the lighting, heating and cooling energy consumption, electric demand and visual comfort of different control strategies. The results showed that integrated controls achieve the lowest total energy in all cases. In most cases, Strategy 6 (Fully integrated lighting and daylighting control with blind tilt angle control without blind height control) achieves the lowest total energy. In mixed humid climates and buildings with interior blinds, Strategy 7 (Fully integrated lighting and daylight control with blind tilt angle and height control) achieves the lowest total energy.

Koo et al. [97], proposed a new method of blind control to maximise the comfort of the user and minimise energy consumption for heating on a clear day.

Palmero-Marrero and Oliveira [98] studied the effect of the louvre shading devices applied to different facades of a building at different latitudes. The results showed that the integration of louvre shading devices offered thermal comfort inside a building and could lead to significant energy savings, compared with a similar building without this type of shading devices.

Along these lines Leung et al. [99]showed that thereflective louvre system can increase working plane illuminance by up to 70% on a clear day. However this system did not generate reasonable savings in costs and presented the disadvantage of creating contrast. DattaIt [100]proved that external fixed horizontal louvres are effective not only in reducing the cooling loads in a building in the summer but also offer a reduction in the global yearly primary energy loads.

Athienitis and Tzempelikos [101]presented a methodology for a combined lighting-daylighting numerical simulation of an office space with an advanced window system incorporating motorized reflective blinds between the two panes. The energy savings using the methodology presented for the particular window system with integrated blinds may exceed 75% for overcast days and 90% for clear days, compared with the case of an office space with no daylighting /dimming control. Also, proper control of the blinds blocks direct solar radiation and reduces glare.

One disadvantage of louvres and blinds is that, if they are controlled manually by the occupants of a building, according to personal preferences, they often do not comply with the thermal, lighting and visual efficiency requirements [102,103,104,105,106,107,108]**.** The occupants may be out of the room when the blinds require adjustment. Furthermore, the occupants often close the louvres or blinds completely to avoid overheating and glare [95,109], reducing in this way the quantity of light. If this occurs, electrical energy consumption for both lighting and cooling will increase [110]. The occupants can also alter the position of the blinds to protect the space from direct sunlight, but they do not often readjust the position of the blinds in the absence of direct sunlight [90,101,102,111,112]**.**

The solution to this problem lies in the use of automated blinds with an appropriate automated control system [102], which helps reach a balance between the right amount of natural light and maximum protection against overheating [94,95,97,105,113,114,115]**.** The advantages of automated blinds are as follows:

* They provide higher levels of natural light and better protection against overheating and glare inside a building [93]**.**
* Better thermal efficiency and higher natural light penetration leading to savings in both cooling loads and lighting energy [93,95,106,116]. Galasiu et al. [117] presented the field-measured performance of two commercial photocontrolled lighting systems, continuous dimming and automatic on/off, as a function of various configurations of manual and photocontrolled automated venetian blinds. The results showed that under clear sky and without blinds both lighting control systems reduced the energy consumption for lighting on average by 50–60% when compared to lights fully on from 6 am to 6 pm. These savings, however, dropped by 5–45% for the dimming system, and by 5–80% for the automatic on/off system with the introduction of various static window blind configurations. The savings in lighting energy were more significant when the lighting control systems were used together with photocontrolled blinds. This was due to the capability of the blinds to adjust their position automatically in direct response to the variable daylight levels. Lee et al. [118], designed a dynamic venetian blind and dimmable electric lighting system to optimize daylight admission and solar heat gain rejection in real-time, while accommodating other occupants’ considerations. The authors showed a significant energy saving (22-86%) and a reduction in peak demands (18-32%) using the automated venetian blind/lighting system instead of static venetian blinds with the same dimmable electric lighting system.
* They close automatically when the temperature inside a building or the levels of light become too high, and they reopen when the temperature and light decrease, to allow penetration of daylight [119]**.**
* The control system adjusts automated blinds to block direct sunlight, avoiding in this way glare, and offering total daylight illumination and electrical illumination on the illumination level range of [102,104]**.**

Ji -Hyun et al. [120], set out to decide whether the environmental performance of a building could be improved through the use of an automated venetian blind when compared with a manual or motorised blind and whether the occupants would feel discomfort when using an automated blind during the summer months. In terms of energy consumption for cooling, automated blinds reduced this consumption compared to fully-opened manual blinds as the automated blinds blocked solar radiation according to the outdoor weather conditions while consuming more energy compared to manual blinds which is fully closed. However, if the additional energy consumption for lighting needed due to the interception and blocking of sunlight is considered, the overall environmental performance of the automated blinds is nearly equal to that of manual blinds when fully opened. As the room illuminance level continuously exceeded the upper limit of 3340 lux., it would be reasonable to assume that the blinds ought to have been fully closed and artificial lighting used. Furthermore, if the additional energy consumption for lighting is considered, the overall environmental performance of the automated blinds is better than that of manual blinds when fully closed. As for the comfort of the occupants, in the case of the automated blinds, the slat angle is controlled to cut off direct sunlight, which reduces the discomfort from excessive solar radiation and direct sunlight. In addition, daylight can be introduced to provide a feeling of openness.

* 1. **Top-lighting systems**

Typical top-lighting systems are:

* Skylight
* Roof monitor
* Sawtooth
* Light pipe

Garcia-Hansen et al. [121], outline the possible energy savings and greater efficiency obtained through the use of top-lighting systems (skylights, roof monitors and clerestory roof windows) in cold areas of the typically template climate of Argentina. The results indicate that heating, ventilation and lighting costs can be significantly reduced through the implementation of these passive solar systems.

* + 1. **Skylight systems**

A skylight system consists of a horizontal or sloping opening in the roof of a building. It is designed to capture sunlight when the sun is at its zenith, allowing daylight to penetrate into buildings. This system of natural illumination can only be used on the top floor of a multi-storey building or in single-storey buildings [122]**.**

To quantify the efficiency of these skylights, some studies employ scale models [123] or computer simulators [124,125]. In this way, Henriques et al. [126] developed a skylight system which responded to the environmental demands of a building’s exterior as well as its interior. Parametric and environmental software analysis was used to generate and assess solutions. Acosta et al. [127] conducted an analysis in order to determine the most suitable set up for a skylight system, in order to ensure maximum working plane illuminance within a room. Treado et al. [48] concluded that skylights are the most efficient option for minimizing total energy use in a building for heating, cooling and lighting. They are furthermore the most effective source of natural lighting, achieving a reduction of 77% in electrical energy consumption. Although, for Al-Obaidi et al. [128] the use of this system is limited to specific climatic regions because of its considerable effect on the indoor environment.

Other researchers have based their studies on the classic treatises dealing with daylight [129]. In this way Tsangrassoulis and Santamouris [130] offer a practical methodology to estimate the efficiency of this system and determine the quantity of light reaching the interior of a building where these devices have been installed. This methodology is based on the flux transfer approach, used to model the distribution of light energy in round skylights of different proportions of height and width, wall reflectance and transmittance of the glass. Chel et al. [131] throughthe study and validation of a model used to estimate daylight factors, showed a potential yearly saving in electrical energy for lighting of 973 kWh/year. This saving is equivalent to 1,526 kg/year of CO2 emissions.

* + 1. **Roof monitor and sawtooth systems**

Roof monitors and sawtooth are lighting systems which differ mainly in form. They consist of vertical or sloping openings in the roof used to capture light. These openings can be designed to reflect sunlight at certain moments of the day or the year, depending on the requirements of a building. The roof monitor system allows sunlight to penetrate a room in winter when the sun is low in the sky, but not during the summer months.

Heras et al. [132]present the experimental results and the specific analysis of thermal energy savings carried out to analyse energy efficiency in a building with a sawtooth system installed.

* + 1. **Light pipe systems**

The light pipe system consists of a dome skylight (to capture sunlight), a reflective tube (to reflect the sunlight to interior spaces) and a diffuser assembly (placed inside the room to be lit). The dome must be ultraviolet and impact resistant, to protect the tube from dust and rain. Commonly two types of light pipe system are used: straight and elbow bends [133]**.**

The light pipe system is an energy-saving technology offering the possibility of illuminating even the farthest depths of an interior space. Darula et al. feel that straight light tubes offer a unique opportunity for carrying natural light to the farthest corners of a room even in spaces with no windows. [134]. However, for Kocifaj et al. [135] the light tube must be pointing directly at the sun to reach its full efficiency potential. Wong and Yang [136] demonstrated that light pipe system can work in both clear and overcast sky conditions. However, there are limiting factors that affect the performance of it such as orientation, solar azimuth angle and angle of incident light.

Görgülü and Ekren [137] lighted a windowless room with a light tube and dimmable electronic ballasts. A saving of around 30% was made using the proposed controller. In the summer months, the energy saved on illumination would be greater.

Jenkins and Muneer [138,139,140] discussed numerous design models/methods to use in predicting light levels in light tubes, in other words, a tool to quantify the best configuration for light tubes in any given situation. A year later, Jenkins et al. [141] developed a model which employed the cosine law of illumination to trace the distribution of the light diffusing light tube, taking into consideration pipe elbow pieces or bends.

Canziani et al. [16] proved that the light pipe system offers an energy saving potential for both electrical energy (used in artificial illumination) and thermal (heating and cooling) energy. They are furthermore capable of avoiding unwanted phenomenon such as direct irradiation, glare, and overheating. They uniformly distribute sunlight to assure adequate luminous comfort.

The follow table presents a summary of research on natural light controls and guides systems.

Insert Table 1

* + - 1. **Conclusions**
	1. **Major survey findings**

Traditional strategies of sun protection reduce the energy transmission through glazed building components using darkened solar shadings and/or mirror glass. The aim here is to reduce the external heat load resulting from solar irradiation into the building being reflected and/or absorbed in the outer skin. This fails to provide the buildings with sufficient natural daylight. The result is an increased use of energy for electric lighting, so that in terms of total energy consumption in these buildings, the mirror glazing often results in a negative energy balance.

Through a well-designed, controlled use of natural light, employing technologies or systems which ensure the penetration of light throughout the whole building, energy consumption designated to lighting and air conditioning can be kept at a minimum.

In accordance with the research analysed, all of the systems and/or strategies of control and/or guidance of natural light guarantee the penetration of natural light into the building, thus reducing the electrical energy consumption for lighting and cooling. They simultaneously improve the thermal and visual comfort of the users of a building. However numerous studies have also brought to light various disadvantages presented by these systems:

* Skylight systems are inappropriate for direct application in the tropics to balance the thermal and lighting loads. Therefore, these systems should be integrated by using shading, glare protection, proper use of reflective surfaces, reflectors, prisms and multi-pane, using splaying and wells for skylight, as well as double-layered roof system, and taking advantage of different geometries, roof angles, orientations, and complicated roof profiles.
* Light shelves affect the architectural and structural design of a building and must be considered at the start of the design phase as they require a relatively high roof in order to function efficiently. These systems must be specifically designed to fit every window orientation, room configuration and latitude. The performance of light shelves is reduced with Eastern or western orientations and in climates where the conditions are predominantly overcast.
* Prismatic glazing has a negligible effect when the sky is overcast. In such conditions the prismatic plates are placed between two transparent panes of glass at the top of the window.
* The disadvantages of using holograms are twofold. Firstly, holograms reduce transparency in an environment and secondly their excessive cost means that they cannot often be used on a large scale. The disadvantage of mirror glass windows is that they reduce the transmission of energy through the glazed surface. This means that, by reducing the external heat load resulting from solar irradiation into the building being reflected and/or absorbed in the outer skin, energy use for electric lighting is increased.
* The Anidolic ceiling offers high levels of illumination in quantitative terms. However, qualitatively, care must be taken over solar angles where the reflection hub may cause glare. Errors in the size or orientation of the hub may cause undesired reflections, even when the system’s performance is good.
* One disadvantage of louvres and blinds is that, if they are controlled manually by the occupants of a building, according to personal preferences, they often do not comply with the thermal, lighting and visual efficiency requirements. The solution to this problem is automated blinds. These are fitted with an appropriate automated control which helps achieve a balance between the correct amount of natural light and maximum protection from overheating.
* The light pipe system is an energy-saving technology offering the possibility of illuminating even the farthest depths of an interior space. However, the light tube must be pointing directly at the sun to reach its full efficiency potential. Prismatic light pipe can work in both clear and overcast sky conditions. However, there are limiting factors that affect the performance of it such as orientation, solar azimuth angle and angle of incident light.

The following table provides a comparison between the different systems of control and guidance of natural light.

Insert Table 2

* 1. **Future perspectives**
* The correct manipulation and exploitation of the sun and daylight is vital as an energy-saving resource and must be treated as a key element in the development of energy concepts.
* Occupants’ attitudes and preferences pose significant impact on the usage of the proposed control systems and consequently, the optimization of building design and comfort management is yet an open challenge.
* An important trend of the future research must constitute quantification of the energy savings (lighting, heating and cooling) and evaluation of the impact on the occupants’ satisfaction.
* Various simulation techniques that allowing the modeling of buildings with these systems of control and guide need to be future research objectives.

**References**

[1] Meijer F, Itard L, Sunikka-Blank M. Comparing European residential building stocks: performance, renovation and policy opportunities. Building Research & Information 2009;37(5):533.

[2] European Commission & Directorate-General for Energy and Transport (2010a). EU energy and transport in figures.

[3] Huber A, Kortman J, Benito, AM, & Scharp M. Developing and implementing. Effective household energy awareness services 2010.

[4] EUROSTAT (2010). Energy - Yearly statistics 2008.

[5] Ghiaus C, Inard C. Energy and environmental issues of smart buildings, in: A Handbook for Intelligent Building 2004;pp.26–51. Available from: http://www.ibuilding.gr/handbook/ (accessed 26 September 2009).

[6] Janssen R. Towards energy efficient buildings in Europe, in: EuroACE 2004, Available from: http://www.euroace.org (accessed 3 May 2010).

[7] Pérez-Lombard L, Ortiz J, Pout C. A review on buildings energy consumption information, Energy and Buildings 2008;40:394–398.

[8] Directive 2010/31/EU (2010). Energy performance of buildings.

[9] European Commission (2008). Communication from the Commission-Energy efficiency: delivering the 20% target.

[10] <http://www.iea.org/>

[11] Blok K. Enhanced policies for the improvement of electricity efficiencies. Energy Policy 2005;33:1635–41.

[12] Alrubaih MS, Zain MFM, Alghoul MA, Ibrahim NLN, Shameri MA, Omkalthum Elayeb. Research and development on aspects of daylighting fundamentals. Renewable and Sustainable Energy Reviews 2013;21:494–505.

[13] Lancashire DS, Fox AE. Lighting: the way to building efficiency. Consulting-specifying engineer; 1996:p.34–6.

[14] Vine E, Lee E, Clear R, DiBartolomeo D, Selkowitz S. Office worker response to an automated venetian blind and electric lighting system: a pilot study. Energy and Buildings 1998;28:205-18.

[15] Greenup P, Bell JM, Moore I. The importance of interior daylight distribution in buildings on overall energy performance. Renew Energy 2001;22(1–3):45–52.

[16] Canziani R, Peron F, Rossi G. Daylight and energy performances of a new type of light pipe. Energy and Buildings 2004;36 (11):1163–76.

[17] Aries MBC, Newsham GR. Effect of daylight saving time on lighting energy use: a literature review. Energy Policy 2008;36(6):1858–66.

[18] Boyce P, Hunter C, Howlett O. The benefits of daylight through windows. New York: Lighting Research Center: Rensselaer Polytechnic Institute; 2003.

[19] Heschong L. Daylighting and human performance. ASHRAE Journal 2002;44:65–7.

[20] Choi JH, Beltran LO, Kim HS. Impacts of indoor daylight environments on patient average length of stay (ALOS) in a healthcare facility. Building and Environment 2012;50:65–75.

[21] Köster H. Daylighting Controls, Performance and Global Impacts. [Sustainable Built Environments](http://link.springer.com/book/10.1007/978-1-4614-5828-9) 2013:pp. 112-162.

[22] Kim JT, Kim G. Overview and new developments in optical daylighting systems for building a healthy indoor environment, Building and Environment 2010;45:256–69.

[23] Webb AR. Considerations for lighting in the built environment: non-visual effects of light. Energy Build 2006;38(7):721–7.

[24] Hviid C, Nielsen T, Svendsen S. Simple tool to evaluate the impact or daylight on building energy consumption. Solar Energy 2008;82:787–98.

[25] Ihm P, Nemri A, Krarti M. Estimation of lighting energy savings from daylighting. Building and Environment 2009;44:509–14.

[26] Kim JH, Yeo MS, Kim KW, Yang KW, Park YJ, Lee KH. An experimental study for the evaluation of the environmental performance by the application of the automated venetian blind. In: Proceedings of Clima 2007 WellBeing Indoors, Helsinki, Finland; Clima; 2007:pp. 1678–85.

[27] Kristl Z, Kosir M, Lah M, Krainer A. Fuzzy control system for thermal and visual comfort in building. Renewable Energy 2008;33:694–702.

[28] Lee ES, Selkowitz S. The design and evaluation of integrated envelope and lighting control strategies for commercial buildings. ASHRAE Transactions 1995;95(101):326–42.

[29] Roche L. Summertime performance of and automated lighting and blinds control system. Lighting Research & Technology 2002;34:11–27.

[30] Tzempelikos A, Athienitis AK. The impact of shading design and control on building cooling and lighting demand. Solar Energy 2007;81:369–82.

[31] Li DHW, Lam JC. Evaluation of lighting performance in office buildings with daylighting controls, Energy and Buildings 2001;33 (8):793–803.

[32] Li DHW, Lam TNT, Wong SL. Lighting and energy performance for an office using high frequency dimming controls, Energy Conversion and Management 2006;47 (9–10):1133–45.

[33] Chen Y, Liu J, Pei J, Cao X, Chen Q, Jiang Y. Experimental and simulation study on the performance of daylighting in an industrial building and its energy saving potential. Energy and Buildings 2014;73:184–91.

[34] Chirarattananon S, Chaiwiwatworakul P, Pattanasethanon S. Daylight availability and models for global and diffuse horizontal illuminance and irradiance for Bangkok. Renewable Energy 2002;26 (1):69–89.

[35] Park KW, Athienitis AK. Workplane illuminance prediction method for daylighting control systems. Solar Energy 2003;75:277–84.

[36] Mohammad Asif ul Haq, Mohammad Yusri Hassan, Hayati Abdullah, Hasimah Abdul Rahman, Md Pauzi Abdullah, Faridah Hussin, Dalila Mat Said. A review on lighting control technologies in commercial buildings, their performance and affecting factors. Renewable and Sustainable Energy Reviews 2014;33:268–79.

[37] Xue P, Mak CM, Cheung HD. The effects of daylighting and human behavior on luminous comfort in residential buildings: A questionnaire survey. Building and Environment 2014;81:51-9.

[38] Krüger EL, Fonseca SD. Evaluating daylighting potential and energy efficiency in a classroom building. J Renew Sustain Energy 2011;3:063112.

[39] Hourani MM, Hammad RN. Impact of daylight quality on architectural space dynamics Case study: City Mall – Amman, Jordan. Renewable and Sustainable Energy Reviews 2012;16:3579– 85.

[40] DIN 5034 Tageslicht in Innenräumen. (Daylight in interiors). [in German].

[41] BS 8206 Part 2 Lighting for buildings e Part 2: Code of practice for daylighting.

[42] Hraska J. Chronobiological aspects of green buildings daylighting. Renewable Energy xxx 2014: 1-6.

[43] Hraska J. Daylight requirements in sustainable building rating systems. Ingineria iluminatului 2011;13(2):5-11. ISSN 1454-5837.

[44] Khan KS, Kunz R, Kleijnen J, Antes G. Systematic reviews to support evidence-based medicine: How to review and apply findings of healthcare research. London: Royal Society of Medicine Press, 2003.

[45] Pullin AS, Stewart GB. Guidelines for systematic review in conservation and environmental management. Conservation Biology 2006;20:1647–1656.

[46] [Zain-Ahmed](http://www.sciencedirect.com/science/article/pii/S0196890401000073) A, [Sopian](http://www.sciencedirect.com/science/article/pii/S0196890401000073) K, [Othman](http://www.sciencedirect.com/science/article/pii/S0196890401000073) MYH, [Sayigh](http://www.sciencedirect.com/science/article/pii/S0196890401000073) AAM, [Surendran](http://www.sciencedirect.com/science/article/pii/S0196890401000073) PN. Daylighting as a passive solar design strategy in tropical buildings: a case study of Malaysia. [Energy Conversion and Management](http://www.sciencedirect.com/science/journal/01968904). 2002;[43(13](http://www.sciencedirect.com/science/journal/01968904/43/13)):1725-36.

[47] Franzetti C, Fraisse G, Achard G. Influence of the coupling between daylight and artificial lighting on thermal loads in office buildings. Energy and Buildings 2004;36:117–26.

[48] Treado S, Gillette G, Kusuda T. Daylighting with Windows, Skylights, and Clerestories. Energy and Buildings 1984;6:319–30.

[49] Ochoa CE, Capeluto IG. Evaluating visual comfort and performance of three natural lighting systems for deep office buildings in highly luminous climates. Building and Environment 2006;41:1128–35.

[50] Edmonds IR, Greenup PJ. Daylighting in the tropics. Solar Energy 2002;73:111–21.

[51] Sanati L, Utzinger M. The effect of window shading design on occupant use of blinds and electric lighting. Building and Environment 2013;64:67-76.

[52] Freewan AA, Shao L, Riffat S. Optimizing performance of the lightshelf by modifying ceiling geometry in highly luminous climates. Solar Energy 2008;82:343–53.

[53] Freewan AA. Maximizing the lightshelf performance by interaction between lightshelf geometries and a curved ceiling. Energy Conversion and Management 2010;51:1600–04.

[54] Al-Sallal KA. Testing glare in universal space design studios in Al-Ain, UAE desert climate and proposed Improvements. Renewable Energy 2007;32:1033–44.

[55] Soler A, Oteiza P. Dependence on solar elevation of the performance of a lightshelf as a potential daylighting device. Renewable Energy 1996;8:198–201.

[56] Soler A, Oteiza P. Lightshelf performance in Madrid, Spain. Building and Environment 1997;32:87–93.

[57] Daniels K, Bartenbach C. Tageslichtdurchflutung durch Sonnenschutz. Teehnik am Bau 1977;3:291-94.

[58] Critten D L. Light enhancement using E-W aligned long prismatic arrays at high latitude. Sol. Energy 1988;41(6):583-91.

[59] Kurata K. Scale-model experiments of applying a Fresnel prism to greenhouse covering. Sol. Energy 1991:46(1):55-57.

[60] URL: <http://www.solartran.com.au/lasercutpanel.htm>.

[61] Lorenz W. A glazing unit for solar control, daylighting and energy conservation. Solar Energy 2001;70(2):109–30.

[62] Christoffers D. Seasonal shading of vertical south-facades with prismatic panes. Solar Energy 1996;57(5):339-43.

[63] Laouadi A, Saber HH, Galasiu AD, Arsenault C. Optical model for prismatic glazing (1415-RP). HVAC&R Research 2013;19:63–75.

[64] Shehabi A, DeForest N, McNeil A, Masanet E, Greenblatt J, Lee ES, Masson G, Helms BA, Milliron DJ. U.S. energy savings potential from dynamic daylighting control glazings. Energy and Buildings 2013;66:415–23.

[65] Edmonds IR. Performance of laser cut light deflecting panels in daylighting applications. Solar Energy Materials and Solar Cells 1993;29:1-26.

[66] Wagner D. Holographic optical elements (HOE) for high efficiency illumination, solar control and photovoltaic power buildings, acronym high efficiency hoes summary (Public). April 2004.

[67] Breitenbach J, Rosenfeld JLJ. Goniospectrometer measurements of the optical performance of a holograohic optical element. Solar Energy 2000;68(5): 427–37.

[68] Müller HFO. Application of holographic optical elements in buildings for various purposes like daylighting, solar shading and photovoltaic power generation. Renewable Energy 1994;5(Part II):935-41.

[69] James PAB, Bahaj AS. Holographic optical elements: various principles for solar control of conservatories and sunrooms. Solar Energy 2005;78:441–54.

[70] Tholl HD, Kubiza R, Stojanoff CG. Stacked volume holograms a light directing element. Proc. SPIE 2255, Optical Materials Technology for Energy Efficiency and Solar Energy Conversion XIII, 486 1994:486-96. doi:10.1117/12.185391.

[71] Klammt S, Müller H, Neyer A. Advanced daylighting using micro-structured components. TU Dortmund. Proceedings of PLDC, Berlin, 27– 31.10.2009.

[72] Wittkopf SK. Daylight performance of anidolic ceiling under different sky conditions. Solar Energy 2007;81:151–61.

[73] Linhart F, Wittkopf SK, Scartezzini JL. Performance of Anidolic Daylighting Systems in tropical climates–Parametric studies for identification of main influencing factors. Solar Energy 2010;84:1085–94.

[74] Wittkopf SK, Yuniarti E, Soon LK. Prediction of energy savings with anidolic integrated ceiling across different daylight climates. Energy and Buildings 2006;38:1120–29.

[75] Cowrret G, Scartezzini JL, Francioli D, Meyer JJ. Design and assessment of an anidolic light-duct. Energy and Buildings 1998;28:79-99.

[76] Scartezzini JL, Courret G. Anidolic daylighting systems. Solar Energy 2002;73(2):123–35.

[77] Linhart F, Scartezzini JL. Minimizing lighting power density in office rooms equipped with Anidolic Daylighting Systems. Solar Energy 2010;84:587–95.

[78] Vázquez-Moliní D, González-Montes M, Fernández-Balbuena AA, García-Botella A, Pohl W, Galan T, Bernabéu E. Horizontal daylighting system for office buildings. Energy and Buildings 2013;67:525–30.

[79] Tzempelikos A. The impact of venetian blind geometry and tilt angle on view, direct light transmission and interior illuminance. Solar Energy 2008;82:1172–91.

[80] Aleo F, Sciuto S, Viadana R. Solar transmission measurements in outdoor conditions of non-homogeneous shading devices. In: Proceedings of the European conference on energy performance and indoor climate in buildings, Lyon, France, 1994:pp.1074–79.

[81] Tzempelikos A, Athienitis AK. Modeling and evaluation of a window with integrated motorized venetian blinds. In: Proceedings of 3rd ISES World Congress, Gotenburg, Sweden, 2003.

[82] Klems JH, Warner JL. Measurement of bi-directional optical properties of complex shading devices. ASHRAE Transactions 1995;101(1):791–801.

[83] Parmelee GV, Aubele WW. The shading of sunlit glass. ASHVE Transactions 1952;58:377–98.

[84] Pfrommer P, Lomas KJ, Kupke C. Solar radiation transport through slat-type blinds: a new model and its application for thermal simulation of buildings. Solar Energy 1996;57(2):77–91.

[85] Kuhn E. Solar control: a general evaluation method for facades with venetian blinds or other solar control systems. Energy and Buildings 2006;38:648–60.

[86] Simmler H, Binder B. Experimental and numerical determination of the total solar energy transmittance of glazing with venetian blind shading. Building and Environment 2008;43(2):197–204.

[87] Rosenfeld JLJ, Platzer WJ, Van Dijk H, Maccari A. Modeling the optical and thermal properties of complex glazing: overview of recent developments. Solar Energy 2000;69 (6-suppl.):1–13.

[88] Yahoda DS, Wright JL. Methods for calculating the effective long-wave radiative properties of a venetian blind layer. ASHRAE Transactions 2004;110(1):463–74.

[89] Kotey NA, Wright JL. Simplified solar optical calculations for windows with venetian blinds. In: Proceedings of the 31st Conference of the Solar Energy Society of Canada Inc. (SESCI) and 1st Solar Buildings Conference (SBRN), Montreal, Quebec, Canada. 2006.

[90] Andersen M, Rubin MD, Powles RC, Scartezzini J.L. Bidirectional transmission properties of venetian blinds: experimental assessment compared to ray-tracing calculations. Solar Energy 2005;78(2):187–98.

[91] Reinhart CF, Walkenhorst O. Validation of dynamic radiance based simulations for a test office with external blinds. Energy and Buildings 2001;33:683–97.

[92] Campbell NS, Whittle JK. Analyzing radiation transport through complex fenestration systems. In: Proceedings of 5th IBPSA conference, Prague, Czech Republic, 1997:173–80.

[93] Hammad F, Abu-Hijleh B. The energy savings potential of using dynamic external louvers in an office building. Energy and Buildings 2010;42:1888–95.

[94] Saelens D, Parys W, Roofthooft J, Tablada de la Torre A. Assessment of approaches for modeling louver shading devices in building energy simulation programs. Energy and Buildings 2013;60:286–97.

[95] Oh MH, Lee KH, Yoon JH. Automated control strategies of inside slat-type blind considering visual comfort and building energy performance. Energy and Buildings 2012;55:728–37.

[96] Shen E, Hu J, Patel M. Energy and visual comfort analysis of lighting and daylight control Strategies. Building and Environment 2014;78:155-70.

[97] Koo SY, Yeo MS, Kim KW. Automated blind control to maximize the benefits of daylight in buildings. Building and Environment 2010;45:1508–20.

[98] Palmero-Marrero AI, Oliveira AC. Effect of louver shading devices on building energy requirements. Applied Energy 2010;87:2040–49.

[99] Leung TCY, Rajagopalan P, Fuller R. Performance of a daylight guiding system in an office building. Solar Energy 2013;94:253–65.

[100] Datta G. Effect of fixed horizontal louver shading devices on thermal perfomance of building by TRNSYS simulation. Renewable Energy 2001;23:497–507.

[101] Athienitis AK, Tzempelikos A. A methodology for simulation of daylight room illuminance distribution and light dimming for a room with a controlled shading device. Solar Energy 2002;72(4):271–81.

[102] Ruck N, Aschehoug Ø, Aydinli S, Christoffersen J, Courret G, Edmonds I, Jakobiak R, Kischkoweit-Lopin M, Klinger M, Lee E, Michel L, Scartezzini JL, Selkowitz S. Daylight in buildings: a source book on daylighting systems and components: a Report of IEA SHC Task 21 / ECBCS Annex 29. Int Energy Agency; 2000.

[103] Kim J, Park Y, Yeo M, Kim K. An experimental study on the environmental performance of the automated blind in summer. Build Environ 2009;44: 1517-27.

[104] Kuhn TE, Bhler C, Platzer WJ. Evaluation of overheating protection with sunshading systems. Sol Energy 2001;69:59-74.

[105] Lee ES, DiBartolomeo DL, Selkowitz SE. Thermal and daylighting performance of an automated Venetian blind and lighting system in a full-scale private office. Energy Build 1998;29:47-63.

[106] Selkowitz S, Lee ES. Advanced fenestration systems for improved daylight performance. Daylighting’ 98 Conference Proceedings, Ontario, Canada;1998.

[107] Chan YC, Tzempelikos A. Efficient venetian blind control strategies considering daylight utilization and glare protection. Solar Energy 2013;98:241–54.

[108] Guillemin A, Morel N. An innovative lighting controller integrated in a selfadaptive building control system. Energy Build 2001;33:477-487.

[109] Selkowitz S, Lee E. Integrating automated shading and smart glazings with daylight controls. International Symposium on Daylighting Buildings (IEA SHC TASK 31);2004.

[110] Illuminating Engineering Society of North America (IESNA). Recommended practice of daylighting. New York: IESNA Rp-5-99; 1999.

[111] Koo SY, Yeo MS, Kim KW. Automated blind control to maximize the benefits of daylight in buildings. Build Environ 2010;45:1508-1520.

[112] Inoue T, Kawase T, Ibamoto T, Takakusa S, Matsuo Y. The development of an optimal control system for window shading devices based on investigations in office buildings. ASHRAE Trans 1988;94:1034-1049.

[113] Chaiwiwatworakul P, Chirarattananon S, Rakkwamsuk P. Application of automated blind for daylighting in tropical region. Energ Convers Manage 2009;50:2927-2943.

[114] DiBartolomeo DL, Lee ES, Rubinstein FM, Selkowitz SE. Developing a dynamic envelope: lighting control system with field measurements. J Illum Eng Soc 1997;26:146-164.

[115] Klems JH, Warner JL. Solar heat gain coefficient of complex fenestrations with a Venetian blind for differing slat tilt angles. ASHRAE Trans 1997;103:1026-1034.

[116] Roisin B, Bodart M, Deneyer A, D’Herdt P. Lighting energy savings in offices using different control systems and their real consumption. Energ Build 2008;40:514-523.

[117] Galasiu AD, Atif MR, MacDonald RA. Impact of window blinds on daylight-linked dimming and automatic on/off lighting controls. Solar Energy 2004;76:523–44.

[118] Lee ES, DiBartolomeo DL, Selkowitz SE. Thermal and daylighting performance of an automated Venetian blind and lighting system in a full-scale private office. Energy and Buildings 1998;29:47-63.

[119] Galasiu AD, Atif MR, MacDonald RA. Impact of window blinds on daylightlinked dimming and automatic on/off lighting controls. Sol Energy 2004;76:523-544.

[120] Ji-Hyun Kim, Young-Joon Park, Myoung-Souk Yeo, Kwang-Woo Kim. An experimental study on the environmental performance of the automated blind in summer. Building and Environment 2009;44:1517–27.

[121] Garcia-Hansen V, Esteves A, Pattini A. Passive solar systems for heating, daylighting and ventilation for rooms without an equatorfacing façade. Renewable Energy 2002;26:91–111.

[122] Shao L, Elmualim AA, Yohannes I, Mirror lightpipes: daylighting performance in real buildings, Lighting Research and Technology 1998;30(1).

[123] Edmonds IR, Moore GI, Smith GB, Swift PD. Daylight enhancement with light pipes coupled to laser-cut light deflecting materials, Lighting Research and Technology 1995;27(1):27-35.

[124] Tsangrassoulis A, Bourdakis V. Comparison of radiosity and ray-tracing techniques with a practical design procedure for the prediction of daylight levels in atria, Renewable Energy 2003;28:2157–62.

[125] Greenup PJ, Edmonds IR. Test room measurements and computer simulations of the micro-light guiding shade daylight redirecting device. Solar Energy 2004;76:99–109.

[126] Henriques GC, Duarte JP, Leal V. Strategies to control daylight in a responsive skylight system. Automation in Construction 2012;28:91–105.

[127] Acosta I, Navarro J, Sendra JJ. Daylighting design with lightscoop skylights: Towards an optimization of shape under overcast sky conditions. Energy and Buildings 2013;60:232–38.

[128] Karam M. Al-Obaidi, Mazran Ismail, Abdul Malek Abdul Rahman. A study of the impact of environmental loads that penetrate a passive skylight roofing system in Malaysian buildings. Frontiers of Architectural Research 2014;3:178–91.

[129] Hopkinson RG, Petherbridge P, Longmore J. Daylighting, Heinemann, London, 1966.

[130] Tsangrassoulis A, Santamouris M. A method to estimate the daylight efficiency of round skylights. Energy and Buildings 2000;32(1):41–45.

[131] Chel A, Tiwari GN, Chandra A. A model for estimation of daylight factor for skylight: An experimental validation using pyramid shape skylight over vault roof mud-house in New Delhi (India). Applied Energy 2009;86:2507–19.

[132] Heras MR, Jiménez MJ, San Isidro MJ, Zarzalejo LF, Pérez M. Energetic analysis of a passive solar design, incorporated in a courtyard after refurbishment, using an innovative cover component based in a sawtooth roof concept. Solar Energy 2005;78:85–96.

[133] Chirarattananon S, Chedsiri S, Renshen L. Daylighting through light pipes in the tropics. Solar Energy 2000;69(4):331–41.

[134] Darula S, Kocifaj M, Mohelníková J. Hollow light guide efficiency and illuminance distribution on the light-tube base under overcast and clear sky conditions. Optik 2013;124:3165– 69.

[135] Kocifaj M, Kundracik F, Darula S, Kittler R. Availability of luminous flux below a bended light-pipe: Design modelling under optimal daylight conditions. Solar Energy 2012;86:2753–61.

[136] Wong I, Yang HX. Introducing natural lighting into the enclosed lift lobbies of highrise buildings by remote source lighting system. Applied Energy 2012;90:225–32.

[137] Görgülü S, Ekrenb N. Energy saving in lighting system with fuzzy logic controller which uses light-pipe and dimmable ballast. Energy and Buildings 2013;61:172–6.

[138] Jenkins D, Muneer T. Light-pipe prediction methods. Applied Energy 2004;79:77–86.

[139] Jenkins D, Muneer T. Modelling light-pipe performances—a natural daylighting solution. Building and Environment 2003;38:965–72.

[140] Jenkins D, Zhang X, Muneer T. Formulation of semi-empirical models for predicting the illuminance of light pipes. Energy Conversion and Management 2005;46:2288–2300.

[141] Jenkins D, Muneer T, Kubie J. A design tool for predicting the performances of light pipes. Energy and Buildings 2005;37:485–92.